20) **protected mode operation of I-80x86 processor**

- space for physical address is 16Mb

- segments may have variable length (max 64k)

- can start from any address (not just a paragraph address)

- enables multitasking

- offers protection methods between programs running at the same time

21) **memory**